{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Enable Macros","License","Introduction","Establishment Description","Traditional Grease Interceptor","Super Capacity Interceptor","Tools Summary","Traditional Installation Guidan","Super Capacity Installation Gui"],"not_rendered":{"charts":0,"images":16,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Enable Macros","index":0,"n_rows":20,"n_cols":2,"rows_kept":20,"cut":false,"hidden":false,"merged":[[24,2,24,3]]}
[]
[null,"Enable Macros"]
[]
[null,"Before you can use RTI's Grease Management Tool you will need to enable Macros in Excel."]
[]
[]
[" "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Once you have enabled Macros in Excel, continue to the the Grease Management Tool."]

{"sheet":"License","index":1,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":true,"merged":[[26,1,26,2],[26,5,26,6]]}
[]
[null,"RTI's Grease Management Tools"]
[]
[]
[]
[null,"Terms and conditions:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"I agree to these conditions:  "]
[]
[]
[]
["Version 1.0 ",null,null,null,"Expires: "]

{"sheet":"Introduction","index":2,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":true,"merged":[[21,1,21,3]]}
[]
[null,"RTI's Grease Interceptor Sizing Tool"]
[]
[]
[]
[]
[]
[]
[" "]
[]
[null,null,null,null,0]
[]
[]
[]
[null,null,null,null,""]

{"sheet":"Establishment Description","index":3,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":true,"merged":[[35,3,35,4]]}
["Establishment Description"]
[]
[]
[null,null,null,null,null,null,null,"Fixtures","Number"]
[null,null,"Number of Seats:",null,null,null,null,"Floor Drains"]
[]
[null,null,"Establishment Type:",null,null,null,null,"3 Compartment Sinks"]
[]
[null,null,"Establishment Condition:",null,null,null,null,"Pre-rinse Sinks"]
[]
[null,null,"Waste Flow Rate:",null,null,"Liters",null,"Mop Sink"]
[]
[null,null,"Retention Time:",null,null,null,null,"2 Compartment Sink"]
[]
[null,null,"Hours of Operation:",null,null,"Hours",null,"Hand Sinks"]
[]
[null,null,"Grease Trap Volume",null,null,"Liters",null,"Total Flow Rating",null,"L/s"]

{"sheet":"Traditional Grease Interceptor","index":4,"n_rows":49,"n_cols":14,"rows_kept":49,"cut":false,"hidden":true,"merged":[[50,2,50,4]]}
["Traditional Grease Interceptor"]
[]
[]
["Suggested Dimensions of Grease Interceptor based on Sizing Worksheet on Sheet 1"]
[]
[]
["Grease Interceptor Volume (from worksheet)",null,null,null,null,{"$f":"'Establishment Description'!E17","v":0},"Liters"]
["Volume (cubic meters) =",null,null,{"$f":"+F7/1000","v":0},"in Cubic Meters"]
[]
[]
[null,null,null,null,null,null,null,"Profile View of Grease Interceptor"]
[null,null,null,null,"(grade)",null,null,null,null,null,null,null,"0.6m"]
[]
["Tank depth =",null,2,"M"]
["Tank width = ",null,{"$f":"+SQRT((D8/2)/3)","v":0},"M"]
["Tank Length = ",null,{"$f":"3*C15","v":0},"M"]
[null,null,null,null,null,null,null,null,"(liquid level)"]
[]
[]
[]
["NOTES:",null,null,null,{"$f":"C14 &\" m\"","v":"2 m"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+C14-0.2","v":1.8}]
["1.  All dimensions in meters"]
["2.  Drawing Not To Scale"]
["3.  These are suggested values only"]
["4.  Always confirm calculations through",null,null,null,null,null,null,{"$f":"+J30*0.66","v":0},null,null,null,{"$f":"+J30*0.33","v":0}]
["     services of sanitary engineer",null,null,null,null,null,null,null,null,null,null,null,null,"0.3m"]
[]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+C16","v":0}]
[]
[]
[null,null,null,null,null,null,null,"End View of Grease Interceptor"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,{"$f":"+J43+0.5","v":2.2999999999999998}]
[null,null,null,null,null,null,null,null,null,{"$f":"+N22","v":1.8}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+J30/3","v":0}]

{"sheet":"Super Capacity Interceptor","index":5,"n_rows":19,"n_cols":12,"rows_kept":19,"cut":false,"hidden":true,"merged":[[28,2,28,4]]}
["Super Capacity Interceptor"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"Example of a high capacity grease interceptor."]
[]
[null,null,null,null,null,null,"Units are sized based on the desired grease storage capacity and the flow rate (liters/second)."]
[null,null,null,null,null,null,"Always consider using a solids separator in line before the high capacity grease interceptor to "]
[null,null,null,null,null,null,"maximize efficiency."]
[]
[null,null,null,null,null,null,"Typical sizes of super capacity interceptors:"]
[]
[null,null,null,null,null,null,"Capacity",null,"Flow",null,null,"Dimensions"]
[]
[null,null,null,null,null,null,"73 kg",null,2.2000000000000002,"l/s",null,"36\" X 23\" X 23\""]
[null,null,null,null,null,null,"180 kg",null,4.7,"l/s",null,"48\" X 30\" X 30\""]
[null,null,null,null,null,null,"272 kg",null,9.5,"l/s",null,"60\" X 42\" X 42\""]

{"sheet":"Tools Summary","index":6,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":true,"merged":[[6,5,13,7],[6,8,13,10],[3,1,5,1],[3,2,5,4],[3,5,5,7],[3,8,5,10],[6,1,13,1],[7,2,13,4],[18,8,19,10],[20,8,21,10],[20,5,21,7],[20,2,21,4],[14,1,15,1],[14,2,15,4],[14,5,15,7],[14,8,15,10],[16,1,17,1],[16,2,17,4],[16,5,17,7],[16,8,17,10],[25,2,25,4],[18,1,19,1],[20,1,21,1],[18,2,19,4],[18,5,19,7]]}
[]
[null,"Grease Interceptor Tools Summary"]
[]
[null,"Name:","Under the sink Grease Interceptor",null,null,"Traditional Outdoor Grease Interceptor",null,null,"Super Capacity Grease Interceptor"]
[]
[]
[null,"Diagram:"]
[]
[]
[]
[]
[]
[]
[]
[null,"Space Requirements:","Low",null,null,"High",null,null,"Medium"]
[]
[null,"Operational Costs:","High",null,null,"Medium",null,null,"Low"]
[]
[null,"Efficiency:","Low",null,null,"High",null,null,"Highest"]
[]
[null,"Dimensions:"]

{"sheet":"Traditional Installation Guidan","index":7,"n_rows":30,"n_cols":2,"rows_kept":30,"cut":false,"hidden":true,"merged":[[32,2,32,4]]}
["Construction Notes for Traditional Grease Interceptor"]
[]
["1.  Tank shall be made of stainless steel, concrete or other watertight materials.  Fiberglass and plastic may also be OK."]
["2.  Piping shall be minimum 100 mm schedule 40 PVC or ="]
["3.  Sanitary \"T\" inlet and outlet shall be installed 100 mm from inside wall"]
["4.  Outlet \"T\" shall extend to 200 mm from bottom of tank"]
["5.  Baffle wall shall be installed to divide the tank into two compartments (2/3 and 1/3)"]
["6.  Baffle wall shall have a transfer opening or transfer pipe where the pipe inlet is 300 mm from tank bottom"]
["7.  Capacity calculations and structure shall be designed and sealed by a duly licensed sanitary engineer "]
["8.  Access ports shall be installed over the inlet and outlet tees and extend a minimum of 100 mm above final grade or flush with pavement"]
["9.  Access port covers shall be steel and marked \"Grease Interceptor\".  IN traffic areas, a structural engineer shall verify adequate load capacity"]
["10.  Liquid depth of the grease interceptor shall be a minimum of 1.8 meters"]
["11.  Tank installing inspection shall occur prior to final backfill with all piping in place"]
["12.  A leak test shall be performed by filling the tank with water and verifying that the tank is water tight."]
[null,"perform the test by first filling with water, then letting sit for 24 hours.  Then refill to the top and verify the water level does not drop more then"]
[null,"one cm per hour"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Use caution when excavating the tank hole Ensure all workers are briefed on proper safety practices."]

{"sheet":"Super Capacity Installation Gui","index":8,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":true,"merged":[[92,2,92,4]]}
["Construction notes for Super Capacity Grease Interceptors"]
[]
["Installation should utilize a minimum 75 mm connection pipe connected to an air vent.  Review the photos and text below for installation ideas."]